#########################################
######## CONFIGURACOES DO MOTOR
#########################################

[engine]
idle_rpm=950
idle_rpm_torque=100
idle_rpm_curve_bias=0.7
peak_rpm=6750
peak_rpm_torque=240
peak_rpm_curve_bias=0.15
max_rpm=7300
inertia=0.25
friction_torque=20
rotational_friction=0.010
viscous_friction=0.012
use_rpm_limiter=1
rpm_limiter_trigger=7200
rpm_limiter_cutoff_time=0.050
;Idle control: 0 = passive, 1 = active
idle_control=1
max_idle_throttle=1
can_stall=1
stall_sensitivity=0.5
stalled_friction_torque=18
starter_effectiveness=0.7
max_fuel_per_rev=0.017

#########################################
######## CONFIGURACOES DO CAMBIO
#########################################

## manual

[clutch_disk_friction]
max_torque_transfer=235

[manual_gearbox]
num_forward_ratios=5
fwd_ratio_1=3.72
fwd_ratio_2=2.40
fwd_ratio_3=1.77
fwd_ratio_4=1.26
fwd_ratio_5=1.00
reverse_ratio=-3.70
gear_change_time=0.15



#########################################
######## CONFIGURACOES DO DIFERENCIAL
#########################################

[differential]
gearRatio=3.25
//do scania era 6.5, aumentando o valor anda mais rapido

## AS OPCOES ABAIXO NAO ESTAO APLICADAS AINDA

type=viscous
#opcoes: open locked viscous clutch_pack torque_bias

## opcoes para viscous
preload=0
powerStiffness=0.2
coastStiffness=0.2

## opcoes para clutch_pack
clutchPreload=50
clutchPackFriction=0.4
powerAngle=45
coastAngle=80

## opcoes para torque_bias
torquePreload=0
powerRatio=5
coastRatio=5

#########################################
######## CONFIGURACOES DO GIRO DA RODA/DIREÇÃO grau 66
#########################################

[steering]
max_steer_angle=38
toe_angle=0
;Ackerman: 0 = disabled, 1 = enabled
use_ackerman=1

; Generally this will be the center of the last axle
[pos_ackerman]
posY=0.29605
posZ=-1.20251

#########################################
######## CONFIGURACOES DO FREIO
#########################################

[brakes]
max_brake_torque=2000
brake_bias=0.7
handbrake_torque=2000
;Handbrake Axle: 0 = rear only, 1 = front only, middle: both
handbrakeAxle=0

#########################################
######## CONFIGURACOES DOS PNEUS
#########################################

## AS CONFIGURACOES DOS PNEUS NAO  ESTAO PROGRAMADAS AINDA
## NAO ALTERE DAQUI PARA BAIXO

## THESE SETTINGS ARE NOT CODED YET, DO NOT CHANGE BELOW

[tires]
enabled=1
type=parametric
#O PARÂMETRO TYPE PODE SER UM
#DESSES ITENS: flat, lineal, smooth, parametric ou pacejka
#os mais comuns serao parametric e pacejka
#DEIXE SEM CONFIGURAR com enabled=0 ou apague isto do arquivo para usar o padrão do jogo, com a configuração de ônibus/caminhão

#caso use o parametric:
[tires_parametric]
adherentX=0.9
adherentY=0.9
peakX=1.7
peakY=1.1
limitX=3.5
limitY=1.0
A=0.1
B=0
C=0.12
D=0

#caso use o pacejka:
[tires_pacejka]
adherent_u=0.95
stiffness=0.65
shape=1.5
peak_u=1.7
curvature=0.1

#caso use o flat:
[tires_flat]
adherentX=1.1
adherentY=1.5

#caso use o smooth:
[tires_smooth]
adherentX=0.5
adherentY=0.95
peakX=1.5
peakY=1.1
limitX=4
limitY=0.8

#caso use o lineal, é parecido com o smooth mas com dados brutos
[tires_lineal]
adherentX=0.5
adherentY=0.95
peakX=1.5
peakY=1.1
limitX=4
limitY=0.8