#########################################
######## CONFIGURACOES DO MOTOR
#########################################

[engine]
idle_rpm=600
idle_rpm_torque=100
idle_rpm_curve_bias=0.3
peak_rpm=2250
peak_rpm_torque=1100
peak_rpm_curve_bias=0.02
max_rpm=2200
inertia=2
friction_torque=50
rotational_friction=0.67
viscous_friction=0.05
use_rpm_limiter=1
rpm_limiter_trigger=6000
rpm_limiter_cutoff_time=0.075
;Idle control: 0 = passive, 1 = active
idle_control=1
max_idle_throttle=1
can_stall=1
stall_sensitivity=0.301
stalled_friction_torque=1000
starter_effectiveness=1
max_fuel_per_rev=0.7

#########################################
######## CONFIGURACOES DO CAMBIO
#########################################

## manual

[clutch_disk_friction]
max_torque_transfer=950

[manual_gearbox]
num_forward_ratios=6
fwd_ratio_1=7.72
fwd_ratio_2=4.42
fwd_ratio_3=2.86
fwd_ratio_4=1.92
fwd_ratio_5=1.3
fwd_ratio_6=1.0
reverse_ratio=-7.1
gear_change_time=0.5



#########################################
######## CONFIGURACOES DO DIFERENCIAL
#########################################

[differential]
gearRatio=6.5
//do scania era 6.5, aumentando o valor anda mais rapido

## AS OPCOES ABAIXO NAO ESTAO APLICADAS AINDA

type=viscous
#opcoes: open locked viscous clutch_pack torque_bias

## opcoes para viscous
preload=100
powerStiffness=0.2
coastStiffness=0.2

## opcoes para clutch_pack
clutchPreload=50
clutchPackFriction=0.4
powerAngle=45
coastAngle=80

## opcoes para torque_bias
torquePreload=0
powerRatio=5
coastRatio=5

#########################################
######## CONFIGURACOES DO GIRO DA RODA/DIREÇÃO
#########################################

[steering]
max_steer_angle=35
toe_angle=0
;Ackerman: 0 = disabled, 1 = enabled
use_ackerman=1

; Generally this will be the center of the last axle
[pos_ackerman]
posY=0.52
posZ=-2.88

#########################################
######## CONFIGURACOES DO FREIO
#########################################

[brakes]
max_brake_torque=20000
brake_bias=0.7
handbrake_torque=10000
;Handbrake Axle: 0 = rear only, 1 = front only, middle: both
handbrakeAxle=0

#########################################
######## CONFIGURACOES DOS PNEUS
#########################################

## AS CONFIGURACOES DOS PNEUS NAO  ESTAO PROGRAMADAS AINDA
## NAO ALTERE DAQUI PARA BAIXO

## THESE SETTINGS ARE NOT CODED YET, DO NOT CHANGE BELOW

#[tires]
#type=pacejka

#[tires_pacejka]
#adherent_u=0.95
#stiffness=0.8
#shape=1.5
#peak_u=1.1
#curvature=-2
