This file provides run settings for the SOLWEIG run initiated at: Fri, 21 Jul 2023 18:09:29
Version: SOLWEIG v2022a

SURFACE DATA
Digital surface model (DSM): /Users/casparraap/Desktop/Uni_2/Bachelor/GIS_Daten/BA/bg_dsm.tif
Model domain: rows = 307, columns = 318
Projected reference system: ETRS89 / UTM zone 32N
Geographical coordinate system: ETRS89
Latitude: 51.310842814473226
Longitude: 9.49171790932668
UTC: 0.0
Transmissivity of light through vegetation: 0.03
Digital vegetation canopy model (CDSM): /Users/casparraap/Desktop/Uni_2/Bachelor/GIS_Daten/BA/CDSM.tif
Trunkzone estimated from CDSM
Trunkzone as percent of canopy height: 0
Landcover scheme active. Parameters taken from: /Users/casparraap/Library/Application Support/QGIS/QGIS3/profiles/default/python/plugins/UMEP-processing-main/processor/landcoverclasses_2016a.txt
Landcover grid: /Users/casparraap/Desktop/Uni_2/Bachelor/GIS_Daten/BA/landcover.tif

DEM used to identify buildings

METEOROLOGICAL FORCING DATA
Meteorological file: /Users/casparraap/Desktop/Uni_2/Bachelor/GIS_Daten/ERA5_1-6-22_1-8-22/ERA5_UTC-51.375N-9.5E-437.6A_2022_200_201_data_60.txt
Diffuse and direct shortwave radiation estimated from global radiation

HUMAN EXPOSURE PARAMETERS
Absorption, shortwave radiation: 0.7
Absorption, longwave radiation: 0.95
Posture of human body: Standing
ENVIRONMENTAL PARAMETERS
Albedo of walls: 0.2
Albedo of ground (not used if land cover scheme is active): 0.15
Emissivity (walls): 0.9
Emissivity of ground (not used if land cover scheme is active): 0.95

ADDITIONAL SETTINGS
Human considered as a standing cylinder
Anisotropic sky diffuse shortwave (Perez et al. 1993) and longwave (Martin & Berdahl, 1984) radiation
