The Belug tables : the basics.

The idea came from http://www.michlug.org/resources/tabledrawings/
Belug adepted the drawings to European sizes (mm <> inch) and available material.

Our basic table is based on 3 by 3 baseplates of 32 studs.
One baseplate is 255.5 mm x 3 = 766.5 mm. We use 766 mm.
In our first version we used 768mm (256 x 3), but after 5 tables we had 1 cm of table left, without baseplate.

The tables are made of 8mm MDF wood.

Our basic height is 70 cm. This makes our legs 69.2 cm + 0.8 cm from our table MDF plate.

The support arround the tables are made of 18mm MDF, sawed in strokes of 40mm in height.
The fully made table is 40mm + 8mm = 48mm => 5 lego bricks in height.

By laying table above each other we can make level of 5 bricks.

We use also different legs, always in steps of 48mm in height.

In the table legs are also extra holes for mounting the tables in depth, to create levels like water, valleys. 
This holes are also 48 mm from center to center.

We use 8mm holes and 6mm bolts. This is necesary for an easy assembly.
The position of the holes is not 100% correct. By using slightly bigger holes, we have 2mm space.

If you have more questions, pleas ask.
If you want some photo's, no problem.
www.belug.be / Contact Us

PS. all the drawings comments are written in Dutch, but since they are technical drawings, it should be clear to read them.
A small translation file is available on Brickshelf